Late PO issuance

EPCC Late PO issuance

CIDB - COA imposed new requirement.

BOMBA Requirement

Unfamiliar with regulatory requirement

AOC/COC/ACC Pumps(Low Shear requirement)

Preference project requirement is not aligned (e.g. Partial Stroke Requirement for EIV)

MVL

Best Practice:

Adjacent parallel pipe rack & sleepers can be merged.

Best Practice:

Use of GRP for seawater intake pipe

Pipe crossing bund / dykewall

Pipe rack design

Best Practice: Simplified concept of pipe rack to improve constructability.

Pipe supplier unable to meet pipe demand.

EPCC Contractor holds back on the issuance of piled foundation drawings for pipe rack, equipment foundations and pipe sleeper.

Best Practice: Sequential erection on Main Pipe rack

Best Practice: Civil: Improve design pipe rack foundation